**SEE-IT assessment form**

|  |  |
| --- | --- |
|  **Assessment instructions**1. **Choose** if you want to assess a full colour or greyscale version of the artwork
2. **Mount** the artwork **on a wall** or a shelf at eye-level.
3. **Lay a tape measure** out on the floor, so that the metal end is touching the wall. Press the button to lock the tape measure off.
4. **If you wore any glasses** for the calibration, wear the same ones for this assessment.
5. **Determine** which particular feature on the artwork you want to assess, e.g. a particular piece of text of graphics.
6. **Choose** if you want to assess reading, recognising or distinguishing.
7. **Walk** backwards and forwards until you find the furthest distance at which the feature is comfortable to read/recognise/distinguish.
8. **Record** below the position of your big toe on the tape measure (in cm). This is your **Assessment Distance**.
9. **Calculate** the corresponding exclusion and colour band using the SEE-IT tool.
 | **Insert a picture of your artwork, or describe it here:** |
| **Assessor 1** | **Assessor 2** |
| Name : | Name: |
| Calibration distance (cm): | Calibration distance (cm): |
| **Feature being assessed** | **Did you read, recognise** **or distinguish?** | **What makes this feature** **difficult to see?** | **Assessment distance (cm)** | **Exclusion (%)****(Colour band)** | **Assessment distance (cm)** | **Exclusion (%)****(Colour band)** |
|  |  |   |   |   |   |   |
|  |  |   |   |   |   |   |
|  |  |   |   |   |   |   |
|  |  |  |  |  |  |  |

**How could the design be improved?**